# Monitoring system

Higher level conditions should be monitored. Ex: is the oscillator ok? Then we need to check a number of items: pump laser status, mode locking, spectrum, and oscillator power. Pump laser status is in this case another monitor object checking: pump power, pump temperature, pump state.

Each monitor object needs a list of parameters (power, spectrum…). They could be updated in qt slots by qt signals.